TMS Signal Generator Signals
============================

AWG	PUPE		Description
===================================
1	Ana1-a		Sigma
2	Ana1-b		DeltaX = 0.2 * Sigma;
3	Ana1-b		DeltaY = -0.1 * Sigma;
4	RefClk		SYSTEM_CLOCK
5	T7		FREF = 470KHz square (should this be pulsed ?)
6	T5		Injection (or SYSTEM_CLOCK = 10MHz square ??)
7	T6		H_CHANGE =  +ve pulse 100ns 
8	T1		CYCLE_START = +ve pulse 100ns
Marker	T2		CYCLE_END =  +ve pulse 100ns

Timing Panel to PUPE
=====================
T1	J26
T2	J19	CYCLE_START
T3	J13	CYCLE_END
T4	J20	CAL_START
T5	J17	CAL_END
T6	J22	INJECTION
T7	J16	H_CHANGE
T8	J27	FREF
